Issued to:		CIXI DIBO ELECTRONICS CO.,LTD	
		NO.235 South Lujia Road, Changhe Town
Cixi
ZHEJIANG 315300 CHINA	
			
This is to certify that
representative samples of		COMPONENT - TERMINAL BLOCKS 	
		See Addendum Page	
			
		Have been investigated by UL in accordance with the Standard(s) indicated on this Certificate.	
			
Standard(s) for Safety:		UL1059, Terminal Blocks.
CAN/CSA C22.2 No. 158-10, Terminal Blocks.	
Additional Information:		See the UL Online Certifications Directory at www.ul.com/database for additional information	

Only those products bearing the UL Certification Mark should be considered as being covered by UL's Certification and Follow-Up Service.

The UL Recognized Component Mark generally consists of the manufacturer’s identification and catalog number, model number or other product designation as specified under “Marking” for the particular Recognition as published in the appropriate UL Directory.  As a supplementary means of identifying products that have been produced under UL’s Component Recognition Program, UL’s Recognized Component Mark: , may be used in conjunction with the required Recognized Marks.  The Recognized Component Mark is required when specified in the UL Directory preceding the recognitions or under “Markings” for the individual recognitions.

Recognized components are incomplete in certain constructional features or restricted in performance capabilities and are intended for use as components of complete equipment submitted for investigation rather than for direct separate installation in the field.  The final acceptance of the component is dependent upon its installation and use in complete equipment submitted to UL LLC.

Look for the UL Certification Mark on the product.

This is to certify that representative samples of the product as specified on this certificate were tested according to the current UL requirements.

Series DB126V, DB126R, DB127V, DB128H, DB128L, DB103, DB301R, DB301V, followed by -5.0 or -5.08, followed by -02 thru -24P or blank, followed by 10, 20, 30, 40, 50, 60, 70, 80, 90 or blank, followed by three alphanumeric or blank.

Series DB128R, DB128V, followed by -5.0 or -7.5, followed by -02 thru -24P or blank, followed by 10, 20, 30, 40, 50, 60, 70, 80, 90 or blank, followed by three alphanumeric or blank.

Series DB2EK, followed by -3.5 or -3.81, followed by -02 thru -24P or blank, followed by 10, 20, 30, 40, 50, 60, 70, 80, 90 or blank, followed by three alphanumeric or blank.

Series DB2EK, DB2EKM, followed by -5.0, -5.08, -7.5 or -7.62, followed by -02 thru -24P or blank, followed by 10, 20, 30, 40, 50, 60, 70, 80, 90 or blank, followed by three alphanumeric or blank.